|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Unit Load Containers**  | **Interchangeability**  | **Usable Volume**  | **Max. net weight capacity**  | **IATA code:**  | **IATA rate class**  | **Dry ice Capacity**  |
| **LD-3 Container** **tools_ShowLetter_006** | 74F / D1F / 743 / 767 / 777 / M 11 / 330 / 340 / truck Loadable on 767 instead of 2 LD2 units | 4.2 m3 / 148 cu. ft | 1,500 kg/ 3,307 lbs | AVE, AKE, XKG, XKN | 8 | - |
| **LD-2 Container** **tools_ShowLetter_004** | 767 / 777 / truck | 3.4 m3 / 120 cu. ft | 1162 kg/ 2561 lbs | DPE | 8 | - |
| **LD-8 Container** **tools_ShowLetter_003** | 767 / 777 / truck | 7,2 m3 / 253 cu. ft | 2342 kg/ 5163 lbs | ALE | 6 | - |
| **LD-9 Envirotainer cooltainer****tools_ShowLetter_007** | 74F / D1F / 743 / 767 / 777 / M 11 / 330 / 340 / truck | 8.3 m3 / 293 cu. ft | 5,588 kg/ 12,319 lbs | RAP | 5 | 300 kg |
| **LD-3 Envirotainer cooltainer****tools_ShowLetter** | 74F / D1F / 743 / 767 / 777 / M 11 / 330 / 340 / truck Loadable on 767 instead of 2 LD2 units | 3.1 m3 / 109 cu. ft | 1,331 kg/ 2,934 lbs | RKN | 8 | 180 kg |
| **LD3-45 Container** **tools_ShowLetter_005** | A319 / A320 / A321 /truck | 3.5 m3 / 124 cu. ft | 1,052 kg/ 2,323 lbs | AKH DKH | Not available | - |
| Weights depend on the structural weight limitations of the different pallet /container positions in the aircraft. Container sizes may vary depending on Carrier equipment. |