|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| **Unit Load Containers** | **Interchangeability** | **Usable Volume** | **Max. net  weight capacity** | **IATA code:** | **IATA rate  class** | **Dry ice  Capacity** |
| **LD-3 Container**  **tools_ShowLetter_006** | 74F / D1F / 743 / 767 / 777 / M 11 / 330 / 340 / truck  Loadable on 767 instead of 2 LD2 units | 4.2 m3 /  148 cu. ft | 1,500 kg/  3,307 lbs | AVE,  AKE,  XKG,  XKN | 8 | - |
| **LD-2 Container**  **tools_ShowLetter_004** | 767 /  777 /  truck | 3.4 m3 /  120 cu. ft | 1162 kg/  2561 lbs | DPE | 8 | - |
| **LD-8 Container**  **tools_ShowLetter_003** | 767 /  777 /  truck | 7,2 m3 /  253 cu. ft | 2342 kg/  5163 lbs | ALE | 6 | - |
| **LD-9 Envirotainer cooltainer**  **tools_ShowLetter_007** | 74F / D1F / 743 / 767 / 777 / M 11 / 330 / 340 / truck | 8.3 m3 /  293 cu. ft | 5,588 kg/  12,319 lbs | RAP | 5 | 300 kg |
| **LD-3 Envirotainer cooltainer**  **tools_ShowLetter** | 74F / D1F / 743 / 767 / 777 / M 11 / 330 / 340 / truck  Loadable on 767 instead of 2 LD2 units | 3.1 m3 /  109 cu. ft | 1,331 kg/  2,934 lbs | RKN | 8 | 180 kg |
| **LD3-45 Container**  **tools_ShowLetter_005** | A319 /  A320 /  A321 /truck | 3.5 m3 /  124 cu. ft | 1,052 kg/  2,323 lbs | AKH  DKH | Not available | - |
| Weights depend on the structural weight limitations of the different pallet /container positions in the aircraft. Container sizes may vary depending on Carrier equipment. | | | | | | |